## Summary

This processor generates and transmits SNMP Traps to the specified SNMP manager. Attributes can be given as processor properties, either predefined or dynamically using Expression Language from flowfiles. Flowfile properties with snmp prefix (e.g. snmp$1.2.3.4.5 - OID) value can be used to define additional PDU variables.

The allowable Generic Trap Types are:

0. Cold Start
1. Warm Start
2. Link Down
3. Link Up
4. Authentication Failure
5. EGP Neighbor Loss
6. Enterprise Specific

Specific trap type can set in case of Enterprise Specific generic trap type is chosen.