## Summary

This processor sends SNMP set requests to a SNMP agent in order to update information associated to a given OID. This processor supports SNMPv1, SNMPv2c and SNMPv3. The component is based on SNMP4J.

The processor constructs SNMP Set requests by extracting information from FlowFile attributes. The processor is looking for attributes prefixed with snmp$. If such an attribute is found, the attribute name is split using the $ character. The second element must respect the OID format to be considered as a valid OID. If there is a third element, it must represents the SMI Syntax integer value of the type of data associated to the given OID to allow a correct conversion. If there is no third element, the value is considered as a String and the value will be sent as an OctetString object.